,Part No.##OTHER##,Model##OTHER##,Manufacturer##OTHER##,Length##LENGTH##MILLIMETERS,Width##LENGTH##MILLIMETERS,Lamp Wattage##OTHER##,Wattage##ELECTRICAL_WATTAGE##WATTS,Voltage##OTHER##,Smart##OTHER##,Photometric Web File##OTHER##,None##OTHER##,Material Luminaire Body##OTHER##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,URL##OTHER##,Lens Type##OTHER##,Lamp##OTHER##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Description##OTHER##,Control Gear##OTHER##,Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES


116w LED - Smart,CX14642DF,Canolux LED,Thorlux Lighting,593,343,116w,125,230v,1,CX14642.IES,"䕉乓㩁䵌㘭ⴳ㤱㔹਍呛卅嵔㘠†奂›䡔⽘啌㙍〵㈯〰ള嬊䅄䕔⁝ㄲㄮ⸰〲〱਍䵛乁䙕䍁⁝桔牯畬⁸楌桧楴杮਍䱛䵕䅃嵔䌠ㅘ㘴㈴਍䱛䵕义䥁䕒⁝䅃低啌⁘䕌⁄䕒䕃卓䑅਍䱛䵁䍐呁⁝㐵堠㈠⁗䕌卄਍䥔呌丽乏൅ㄊ㤠㈱‰⸹㈱㌠‷‷‱′㈮㜸⸠㘲‶രㄊ〮‰⸱〰ㄠ〳਍‰‵〱ㄠ‵〲㈠‵〳㌠‵〴㐠‵〵㔠‵〶㘠‵〷㜠‵〸㠠‵〹㤠‵〱‰〱‵ㄱ‰ㄱ‵㈱‰਍㈱‵㌱‰㌱‵㐱‰㐱‵㔱‰㔱‵㘱‰㘱‵㜱‰㜱‵㠱‰਍‰㔱㌠‰㔴㘠‰㔷㤠‰਍㐵⸵″㐵⸱‸㈵⸱‸ㄵ⸱‸㤴⸶‴㜴⸱‹〴⸷‰㘳⸵‵㠲⸱‶㘱⸳″㌶㤮㌠⸳‹㤱㌮ഠㄊ⸵‸㐲〮ㄠ⸳‷㘱㠮㔠㔮〠㌮〠ㄮ〠ㄮ〠ㄮ〠ㄮ〠ㄮ〠㈮〠㈮〠㌮〠㐮〠㘮〠㜮〠㠮ഠ《㤮ㄠ〮ㄠㄮㄠㄮㄠ㈮ㄠ㈮ഠ㔊㔴㌮㔠㤳㌮㔠ㄲ㤮㔠ㄱ㐮㐠ㄹ㘮㐠ㄷ㜮㐠㈱㐮㌠㔶㐮㈠㈹㤮ㄠ㜶㈮㘠⸷‴㠳㐮㈠⸱‴਍㔱㌮㈠⸲″㘱㐮ㄠ⸴′⸷″⸰″⸰‱⸰‱⸰‱⸰‱⸰‱⸰′⸰″⸰‴⸰‵⸰‶⸰‷⸰‸਍⸰‹⸱‰⸱‱⸱′⸱′⸱′਍㐵⸵″㐵⸸‹㌵⸲‶ㄵ⸶‵〵⸰′㠴⸰‱㌴⸳′㠳⸰′㈳⸸′ㄲ⸰‰㈸㠮㘠⸹‸㈳㌮ഠ㈊⸵″㔱㤮㈠⸳″〱〮ㄠ⸱″⸰″⸰‱⸰‱⸰‱⸰‱⸰′⸰′⸰″⸰‴⸰‵⸰‶⸰‷⸰‸਍⸰‹⸱‰⸱‱⸱′⸱′⸱′਍㐵⸵″㐵⸱‱㈵⸶‴〵⸸‷㠴⸸‰㘴⸶″㐴⸳‸㠳⸶‸㌳⸹‶㐲⸹‹㌱⸲‱㠶㠮㘠⸸‴਍㔵㈮㌠⸸‱㜱ㄮ㈠⸱‱ㄱ㌮〠㠮〠ㄮ〠ㄮ〠ㄮ〠㈮〠㈮〠㈮〠㌮〠㐮〠㔮〠㘮〠㜮〠㤮ഠ《㤮ㄠ〮ㄠㄮㄠ㈮ㄠ㈮ㄠ㈮ഠ㔊㔴㌮㔠㌴㈮㔠〳㘮㔠㌱〮㐠㠸㤮㐠㔶㜮㐠㌴㠮㐠㘱㐮㌠㠵㤮㈠㠹㠮㈠㈱ㄮㄠ㘴㌮㠠⸹‵਍〴㤮㈠⸹‶㈳㤮㈠⸵‱⸸‸⸰‸⸰‱⸰‱⸰‱⸰′⸰′⸰″⸰″⸰‴⸰‵⸰‶⸰‸⸰‹਍⸰‹⸱‰⸱‱⸱′⸱′⸱′਍㐵⸵″㐵⸳‸㈵⸶‴〵⸷‹㠴⸸′㔴⸹‷㌴⸲‷〴⸸′㜳⸲‶ㄳ⸱‰㈲⸹‷㔱⸹‱〱⸰‰਍㜶㌮㌠⸷′㔱ㄮ㔠㠮㌠㐮〠㘮〠ㄮ〠ㄮ〠ㄮ〠㈮〠㈮〠㌮〠㐮〠㔮〠㘮〠㜮〠㠮〠㤮ഠ《㤮ㄠ〮ㄠㄮㄠ㈮ㄠ㈮ㄠ㈮ഠ㔊㔴㌮㔠〴㜮㔠ㄳㄮ㔠㐱㐮㐠㈹㜮㐠㈶㠮㐠ㄴ㘮㐠㤰㜮㌠㤶㌮㌠〰〮㈠㌵㤮ㄠㄸㄮ㤠⸸‴਍㐲㠮㤠〮㜠㔮㘠㐮㌠㘮〠㐮〠ㄮ〠ㄮ〠ㄮ〠㈮〠㈮〠㌮〠㐮〠㔮〠㘮〠㜮〠㠮〠㤮〠㤮ഠㄊ〮ㄠㄮㄠ㈮ㄠ㈮ㄠ㈮ഠ
","Thorlux - Steel, Paint Finish, White, Glossy",11150,www.thorlux.com,Acrylic Cover,LED,4000,LED luminaires with zinc coated steel body and 2.8mm thick acrylic front cover. Recessed or surface mounting options. 'Intelligent' Smart options with integral presence detection.,Smart,125


116w LED - Non- Dimming,CX14641LF,Canolux LED,Thorlux Lighting,593,343,116w,125,230v,0,CX14641.IES,"䕉乓㩁䵌㘭ⴳ㤱㔹਍呛卅嵔㘠†奂›䡔⽘啌㙍〵㈯〰ള嬊䅄䕔⁝ㄲㄮ⸰〲〱਍䵛乁䙕䍁⁝桔牯畬⁸楌桧楴杮਍䱛䵕䅃嵔䌠ㅘ㘴ㄴ਍䱛䵕义䥁䕒⁝䅃低啌⁘䕌⁄䕒䕃卓䑅਍䱛䵁䍐呁⁝㐵堠㈠⁗䕌卄਍䥔呌丽乏൅ㄊ㤠㈱‰⸹㈱㌠‷‷‱′㈮㜸⸠㘲‶രㄊ〮‰⸱〰ㄠ〳਍‰‵〱ㄠ‵〲㈠‵〳㌠‵〴㐠‵〵㔠‵〶㘠‵〷㜠‵〸㠠‵〹㤠‵〱‰〱‵ㄱ‰ㄱ‵㈱‰਍㈱‵㌱‰㌱‵㐱‰㐱‵㔱‰㔱‵㘱‰㘱‵㜱‰㜱‵㠱‰਍‰㔱㌠‰㔴㘠‰㔷㤠‰਍㐵⸵″㐵⸱‸㈵⸱‸ㄵ⸱‸㤴⸶‴㜴⸱‹〴⸷‰㘳⸵‵㠲⸱‶㘱⸳″㌶㤮㌠⸳‹㤱㌮ഠㄊ⸵‸㐲〮ㄠ⸳‷㘱㠮㔠㔮〠㌮〠ㄮ〠ㄮ〠ㄮ〠ㄮ〠ㄮ〠㈮〠㈮〠㌮〠㐮〠㘮〠㜮〠㠮ഠ《㤮ㄠ〮ㄠㄮㄠㄮㄠ㈮ㄠ㈮ഠ㔊㔴㌮㔠㤳㌮㔠ㄲ㤮㔠ㄱ㐮㐠ㄹ㘮㐠ㄷ㜮㐠㈱㐮㌠㔶㐮㈠㈹㤮ㄠ㜶㈮㘠⸷‴㠳㐮㈠⸱‴਍㔱㌮㈠⸲″㘱㐮ㄠ⸴′⸷″⸰″⸰‱⸰‱⸰‱⸰‱⸰‱⸰′⸰″⸰‴⸰‵⸰‶⸰‷⸰‸਍⸰‹⸱‰⸱‱⸱′⸱′⸱′਍㐵⸵″㐵⸸‹㌵⸲‶ㄵ⸶‵〵⸰′㠴⸰‱㌴⸳′㠳⸰′㈳⸸′ㄲ⸰‰㈸㠮㘠⸹‸㈳㌮ഠ㈊⸵″㔱㤮㈠⸳″〱〮ㄠ⸱″⸰″⸰‱⸰‱⸰‱⸰‱⸰′⸰′⸰″⸰‴⸰‵⸰‶⸰‷⸰‸਍⸰‹⸱‰⸱‱⸱′⸱′⸱′਍㐵⸵″㐵⸱‱㈵⸶‴〵⸸‷㠴⸸‰㘴⸶″㐴⸳‸㠳⸶‸㌳⸹‶㐲⸹‹㌱⸲‱㠶㠮㘠⸸‴਍㔵㈮㌠⸸‱㜱ㄮ㈠⸱‱ㄱ㌮〠㠮〠ㄮ〠ㄮ〠ㄮ〠㈮〠㈮〠㈮〠㌮〠㐮〠㔮〠㘮〠㜮〠㤮ഠ《㤮ㄠ〮ㄠㄮㄠ㈮ㄠ㈮ㄠ㈮ഠ㔊㔴㌮㔠㌴㈮㔠〳㘮㔠㌱〮㐠㠸㤮㐠㔶㜮㐠㌴㠮㐠㘱㐮㌠㠵㤮㈠㠹㠮㈠㈱ㄮㄠ㘴㌮㠠⸹‵਍〴㤮㈠⸹‶㈳㤮㈠⸵‱⸸‸⸰‸⸰‱⸰‱⸰‱⸰′⸰′⸰″⸰″⸰‴⸰‵⸰‶⸰‸⸰‹਍⸰‹⸱‰⸱‱⸱′⸱′⸱′਍㐵⸵″㐵⸳‸㈵⸶‴〵⸷‹㠴⸸′㔴⸹‷㌴⸲‷〴⸸′㜳⸲‶ㄳ⸱‰㈲⸹‷㔱⸹‱〱⸰‰਍㜶㌮㌠⸷′㔱ㄮ㔠㠮㌠㐮〠㘮〠ㄮ〠ㄮ〠ㄮ〠㈮〠㈮〠㌮〠㐮〠㔮〠㘮〠㜮〠㠮〠㤮ഠ《㤮ㄠ〮ㄠㄮㄠ㈮ㄠ㈮ㄠ㈮ഠ㔊㔴㌮㔠〴㜮㔠ㄳㄮ㔠㐱㐮㐠㈹㜮㐠㈶㠮㐠ㄴ㘮㐠㤰㜮㌠㤶㌮㌠〰〮㈠㌵㤮ㄠㄸㄮ㤠⸸‴਍㐲㠮㤠〮㜠㔮㘠㐮㌠㘮〠㐮〠ㄮ〠ㄮ〠ㄮ〠㈮〠㈮〠㌮〠㐮〠㔮〠㘮〠㜮〠㠮〠㤮〠㤮ഠㄊ〮ㄠㄮㄠ㈮ㄠ㈮ㄠ㈮ഠ
","Thorlux - Steel, Paint Finish, White, Glossy",11150,www.thorlux.com,Acrylic Cover,LED,4000,LED luminaires with zinc coated steel body and 2.8mm thick acrylic front cover. Recessed or surface mounting options. 'Intelligent' Smart options with integral presence detection.,Non-Dimming,125